SSH Verbindung von pi zu pi

SSH-Verbindung pi mit der IP 192.168.20.212 mit dem Namen raspberrypi nach pi mit der IP 192.168.20.211 mit dem Namen SERVER:

ssh pi@192.168.20.211

Die eventuelle Fehlermeldung bestätigen, danach das Passwort des Users pi am Zielrechner eingeben.

The authenticity of host '192.168.20.211 (192.168.20.211)' can't be established.
ECDSA key fingerprint is SHA256:l0+/zhyEWIDDgj1nHFNm9Atc6/zjfJzEYeu1bvIqsFo.
Are you sure you want to continue connecting (yes/no)? yes

pi@raspberrypi:/home $ pi@192.168.20.211's password:

Linux SERVER 4.19.75-v7l+ #1270 SMP Tue Sep 24 18:51:41 BST 2019 armv7l
The programs included with the Debian GNU/Linux system are free software;
the exact distribution terms for each program are described in the
individual files in /usr/share/doc/*/copyright.
Debian GNU/Linux comes with ABSOLUTELY NO WARRANTY, to the extent
permitted by applicable law.
Last login: Sun Jan 26 17:29:56 2020 from 192.168.20.212
pi@SERVER:~ $

Von hier aus kann man an der Konsole des Zielrechners arbeiten.

Um wieder auf den Ausgangsrechner zu gelangen, den Befehl exit eingeben.